GRATIESTI – STEAUA CALAUZA FACILITY RENOVATION PPROJECT - MOLDOVA
19 Oct 2013
LOCATION:

The existing facility is located in the village of Gratiesti, a few kilometers away from the capital Chisinau.
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EXISTING LAYOUT OF THE FACILITY
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Bathroom: Complete renovation of the room currently used as a warehouse to be converted into a new handicapped rated bathroom. The work shall include:

· New ceramic grès tiles sloped towards a new floor drain. Floor at the entrance door shall be at the same elevation as the floor in the hallway.
· Ceramic tiles on the wall, from the floor to be new ceiling. Use 20x30 cm ceramic tiles. Use combination of 2 colors or two different ceramic tiles.

· Ceiling: Use green type gypsum board rated for humid atmospheres.

· Wall mounted sink

· European standard toilet
· Stainless steel bars for people with limited mobility

· New electric hot water heater (25 liters)

· Automatic hand drier

· All needed accessories such as toilet paper holder, hangers, door stops, etc.
BUDGETARY COST ESTIMATE = $5,000
PICTURES SHOWING EXISTING CONDITIONS
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Location of Gratiesti
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Location of the facility
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In orange the areas under the scope of work of this report 
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Main entrance
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Main facade from main street.











